

**TEP-220M POS Printer Setup**

Download 2 files from <http://www.gainscha.com.cn/download_list.asp?lan=zh-en&skin=4&id=39>



Connect USB cable PC to Printer & Power up the printer.

Go to Devices & Printers and USB Controller should not have a warning sign. If it does, manually update the drivers from the downloaded “USB Virtual COM Driver” file. It should then look like this.



If it shows the com port number (make a note of that for printer setup). If not, then it is a “Virtual USB port” that must be selected during setup.

Restart the PC.

Then install the Printer using the installation Application in the “GP80 Driver” files downloaded. During installation.

It will ask for the series, which is “GP-80250 Series”.

It will ask for the port where the printer is installed.

* If the COM port number was visible in the gprinter USB printer support icon, then use that.
* If the COM port is not displayed, it will be one of the virtual printer ports. (trial n error printing test pages)

Nice video here walks one through the setup: <https://youtu.be/QCryqQzxoa4>